IRGA swap protocol

1. Write down reading from existing IRGA
2. Save config file with date, SN of old IRGA and site abbreviation
3. Swap
4. Load new config file with latest date and correct sn for new IRGA
5. Go to the Calibration menu—put in A0 and A1 pressure settings from licor box
6. Cycle power
7. Check for flags, write down new readings