Spectral protocol

Patty Oikawa

2015.05.29

1. Make sure card is fully inserted
2. Turn on
3. Go to:
	1. Tools
	2. Manual control
	3. Acq parameters
	4. Corrections
	5. Edark=ON
	6. Averages 5
4. Go to Reflectance
	1. connect sensor
	2. Reference—point sensor up and press triangle
	3. Dark—disconnect sensor, put on cap and press dark
5. Sample
	1. Point down, press save—check and make sure recording
	2. Do 2 pointed down
	3. Then do 1 up
	4. Then go back and do reference and dark

Try to take measurements in fully sunny conditions, not foggy or when clouds are passing by changing light a lot